TECHNOZON X11 FASTBOOT DRIVER v1.0.0

1. Extract the ZIP completely.
2. Run INSTALL_DRIVER.cmd.
3. Confirm the Windows User Account Control prompt.
4. After the PASS message, boot the NEXON X11 into fastboot and connect USB A-to-A.

This package installs only the Android Bootloader Interface driver.
It does not flash the TV box, unlock the bootloader, or erase data.

pnputil exit code 259 is not treated as a failure when readback confirms the driver in Windows Driver Store.
