TECHNOZON MODIFIER X11 v1.2.0 RC
================================

RU: Откройте Docs\INSTALL_RU.md и запустите START_RU.cmd.
UK: Відкрийте Docs\INSTALL_UK.md і запустіть START_UK.cmd.
EN: Open Docs\INSTALL_EN.md and run START_EN.cmd.

TARGET / ЦЕЛЬ / ЦІЛЬ
---------------------
Clean NEXON X11 only:
  device: ross
  Android: 14
  build incremental: 250926144031
  bootloader product: kylin / RTD1325

DO NOT use this package on SlimBOX, RT-X2, another X11 build, or another SoC.
The installer checks file hashes, Android properties, and the fastboot product
before restoring verified stock to the inactive init_boot and writing Magisk to the active init_boot.

After installation:
  - TECHNOZON Modifier X11 is production-signed;
  - Magisk 30.7 controls root access;
  - STESH, subscriptions, and TV-box applications are installed as one Magisk module;
  - STESH boot animation, interface performance profile, double-HOME recent apps, Light Sleep, and legacy-su guard are active;
  - TV SMB Manager 1.3.3 provides the SMB/NAS client, DocumentsProvider, seekable playback streaming, and optional Samba server;
  - TV SMB Manager is paired to the production-signed Modifier and this exact X11 profile;
  - the untrusted stock X-plore mod and Aptoide are removed for user 0;
  - Aptoide is removed for Android user 0;
  - unknown-source installers are blocked;
  - TCP ADB port 1325 is closed after reboot by default.
  - Modifier can explicitly keep port 1325 open after reboot, control the double-HOME recent-apps list, and show the active Cyber Stefania wallpaper. UI size and DPI remain under stock firmware control for reliable HDMI sleep/wake behavior.
  - Remote SMB shares are available inside TV SMB Manager and compatible SAF clients. They are not mounted as a global Linux disk because this X11 kernel has no CIFS filesystem support.
  - The Update screen verifies a separately RSA-signed TECHNOZON manifest, exact X11 profile, payload size, SHA-256, APK production signer, and Magisk module id/versionCode before installation. It never flashes bootloader, init_boot, DTB, super, or firmware slots.
    Use this only in a trusted LAN; disable it when maintenance is complete.

For maintenance, connect USB and run:
  Scripts\Enable_Maintenance_TCP_ADB_USB.cmd

To invalidate and recreate the TV SMB pairing, connect USB and run:
  ROTATE_TVSMB_PAIRING_USB.cmd

For stock init_boot rollback, run:
  ROLLBACK_TO_STOCK_X11.cmd

If slot A does not boot and the box still enters fastboot, try:
